
ditv_0004


aareadme.txt
============


calib/
========

 - Labels verified.
 - Tranmission profile tables verified.
 - Question for reviewers:  Should the fixed calibration files for
   each instrument, such as filter transmission profiles or quantum 
   efficiency profiles, reside in four instrument-specific data sets
   or in one instrumental data set?
    

catalog/
========

 - Catalog files verified.
 - Mission, instrument host, and instrument catalog files are minimal
   per MA's request.


document/image_log/
===================

 - Label verified. 
 - An image log in MS Excel format was included because this is the original
   image log.  A PDF version was attempted but information was cropped because
   of the width of the log.  However, a comma-separated, ASCII version is
   included in the archive.


document/pdsdd/
===============

 - Label verified. 
 - Is this the correct way to include a local DD in an archive?


document/reports/
=================

 - Labels verified. 


document/temp_log/
==================

 - Label verified. 
 - The document temp_ext_hri.txt contains an IDL program that was
   used for IR FPA dark current analysis.  Should the program
   be reclassified as software before ingestion?


data/
=====

 - Labels verified.
 - At the Deep Impact science team meeting on 13-14 September 2004, 
   several members requested that the Science Data Center (SDC) modifiy
   all HRIIR image mode 6 FITS data from the thermal-vacuuum test by
   multiplying both the reset and data frames by negative one.  Without
   this modification, the data frame must be subtracted from the reset
   frame to ensure the resulting image had positive data number.  It is
   more intuitive to subract the reset frame from the data frame.  However,
   Mike A'hearn and Stef McLaughlin prefer that the data remain in the
   original state as used by the science team for calibration analyses.


index/
====== 

 - Labels verified.
 - Index tables verified.

